{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["外眼"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"外眼","index":0,"n_rows":34,"n_cols":9,"rows_kept":34,"merged":[[1,0,13,0],[14,0,22,0],[23,0,33,0]]}
["套包名称","器械名称","大致规格型号","单位","数量","产品描述","生产厂家","注册备案号","价格"]
["眼眶手术套包","手术刀柄","3号","把",1,"3号，扁平式，总长125mm。"]
[null,"眼用手术剪","弯尖头","把",1,"眼科剪（弯尖头），总长100mm。"]
[null,"眼用结扎镊","直形","把",1,"别名：大齿镊 齿宽1.0mm　1X2平齿，直横槽手柄，总长105mm.。"]
[null,"眼用止血钳","大号直头","把",1,"网纹型夹持面，指圈型手柄，总长128mm"]
[null,"眼用止血钳","大号弯头","把",1,"弯头，总成125mm。"]
[null,"眼睑拉钩","11.0","把",1,"单头宽11.0mm，总长134mm。"]
[null,"眼睑支持板","弧形","把",1,"头部宽度18mm、21mm，总长110mm。"]
[null,"系线镊","直形","把",1,"6mm直平台，贝尔式手柄，总长110mm."]
[null,"眶睑板","弧形","把",1,"头部宽度18mm、总长110mm"]
[null,"巩膜剥离子","大号","把",1,"不锈钢双头巩膜剥离子，总长182mm"]
[null,"眶睑板","弧形","把",1,"两端头部宽度分别为12mm、11mm，带刻度，总长200mm。"]
[null,"眼睑拉钩","深部拉钩式","把",1,"眼眶深部拉钩，总长144mm。"]
[null,"眼睑拉钩",8,"把",1,"单头宽8.0mm，总长134mm。"]
["玻切手术套包","开睑器","可调式","把",1,"封口式，头部宽11mm， 张开度35mm。"]
[null,"显微眼用镊","内界膜式","把",1,"25G眼底内界膜镊，耐高温医用高分子材料基座，工作长度32mm，需配合手柄使用，非无菌提供，可高温消杀。"]
[null,"眼科手术器械手柄","弧形式","把",1,"波纹爪片，Ø11绿色，眼科手术器械手柄，辅助头部使用。"]
[null,"笛针","25-P","把",1,"25G，工作长度32mm，硅胶软头伸出针管2mm，尾部有软管长110mm配鲁尔双接头，耐高温医用高分子材料手柄，可与设备连接。非无菌提供，可高温消杀。"]
[null,"笛针","25-P","把",1,"25G，总长135mm，工作长度32mm，带内芯，内芯伸出针管0.5mm，耐高温医用高分子材料手柄，非无菌提供，可高温消杀。"]
[null,"显微结扎镊","直形","把",1,"三孔直齿眼用结扎镊,.12mm　1X2平齿，头部6mm台阶，三孔手柄，总长110mm"]
[null,"系线镊","直形","把",1,"系线镊,6mm直平台，贝式手柄，总长105mm"]
[null,"显微眼用持针钳","弯尖头","把",1,"弯尖头，无锁扣，滚花手柄，头部长9.5mm，总长130mm.可用于6-0至10-0缝合线."]
[null,"角膜剪","长刃","把",1,"长刃，弯钝头，刃尖至螺丝中心16mm，总长128mm， 交叉处扭哈夫式。"]
["白内障手术套","开睑器","\\","把",1,"封口式，头部宽11mm， 张开度35mm。"]
[null,"无齿镊","\\","把",1,"6mm直平台，贝尔式手柄，总长110mm."]
[null,"有齿镊","\\","把",1,"1X2平齿，头部6mm台阶，三孔手柄，总长110mm 。"]
[null,"撕囊镊","\\","把",1,"折弯处进入眼睛部分带2.5mm，5mm刻度，直形折弯14mm，圆柄，总长110mm. 1.8mm 微切口专用，带刻度 。"]
[null,"劈核刀","\\","把",1,"45°劈刀，头部长1.5mm，总长118mm。"]
[null,"人工晶体调位钩","\\","把",1,"磨菇头调节杆，头部宽0.7mm，总长120mm。"]
[null,"囊膜剪","\\","把",1,"直尖头，刃尖至螺丝中心长18mm， 哑光，总长128mm。"]
[null,"角膜剪","\\","把",1,"长刃，弯钝头，刃尖至螺丝中心16mm，总长128mm， 交叉处扭哈夫式。"]
[null,"显微眼用持针钳","\\","把",1,"弯尖头，无锁扣，头部长13mm，总长140mm.可同时用于6-0与10-0缝合线。"]
[null,"眼科剪","\\","把",1,"眼科剪（弯尖头），总长100mm。"]
[null,"虹膜恢复器","\\","把",1,"1.25mm×15mm虹膜恢复器，总长118mm。"]